# EQUIPMENT CALIBRATION

## Recommended Equipment Maintenance Protocols:

* Check and adjust any equipment when it has been damaged.
* Check, adjust and perform maintenance on equipment in house at least once per year or send equipment out for adjustment and maintenance at least once per year.
* Follow the manufacturer’s specifications for equipment maintenance schedules and requirements.
* Check and adjust equipment when it is in heavy use.
* Check and adjust equipment when it is coming back into use after being unused for some time.
* Confirm equipment that is new or rented.
* Regularly check and adjust prism poles, tribrachs, etc.
* Maintain a record of checks and adjustments to each piece of equipment, in accordance with Section 1.12 of the National Standards for the Survey of Canada Lands.